You lose fella! The grounding grid is not complying with a safe design. Go back to the design.

The Touch voltage is **23091.52 V** and the tolerable touch voltage is **2166.58 V** On the other hand, the step voltage is 17378.53 V and the tolerable step voltage is 664.68 V.